# Marine Mooring Cleats

# Information Needed for Quotations

See full cleat catalog here:   
<http://www.pacificmarine.net/construction/pier-dock-hardware/marine-cleats.htm>

1. How many cleats do you need?

2. Does cleat need to be rated to hold a specific load? Or unrated?

- Rated

- Unrated

3. What is the length and capacity of the cleat? (Tip to Tip and Metric Tons)

CLAA-XX (where AA is length and XX is capacity)

- 16 inch Unrated 5 8 10 15

- 18 inch Unrated 5 8 10 20

- 24 inch Unrated 5 10 15 20

- 36 inch Unrated 15 20 30 35

- 42 inch Unrated 15 25 30 40

- 50 inch Unrated 15 20 30 40

- 57 inch Unrated 20 30 40 50

4. Are the cleats for:

- new concrete

- existing concrete

- weld down

5. What is the cleat material of construction?

- Steel

- Stainless Steel

6. What is the hardware material of construction?

- Steel

- Steel HDG

- Stainless Steel 304

- Stainless Steel 316

7. What finish is required for the cleat?

- no paint / bare metal

- primer only

- coal tar epoxy

- hot dipped galvanized

8. Location for delivery? (So we can include shipping costs)