# Marine Mooring Cleats

# Information Needed for Quotations

See full cleat catalog here:
<http://www.pacificmarine.net/construction/pier-dock-hardware/marine-cleats.htm>

1. How many cleats do you need?

2. Does cleat need to be rated to hold a specific load? Or unrated?

 - Rated

 - Unrated

3. What is the length and capacity of the cleat? (Tip to Tip and Metric Tons)

 CLAA-XX (where AA is length and XX is capacity)

 - 16 inch Unrated 5 8 10 15

 - 18 inch Unrated 5 8 10 20

 - 24 inch Unrated 5 10 15 20

 - 36 inch Unrated 15 20 30 35

 - 42 inch Unrated 15 25 30 40

 - 50 inch Unrated 15 20 30 40

 - 57 inch Unrated 20 30 40 50

4. Are the cleats for:

 - new concrete

 - existing concrete

 - weld down

5. What is the cleat material of construction?

 - Steel

 - Stainless Steel

6. What is the hardware material of construction?

 - Steel

 - Steel HDG

 - Stainless Steel 304

 - Stainless Steel 316

7. What finish is required for the cleat?

 - no paint / bare metal

 - primer only

 - coal tar epoxy

 - hot dipped galvanized

8. Location for delivery? (So we can include shipping costs)